Tel

[](http://www.redmire.co.uk/)

Tel: 01789 400988

Email: enquiries@redmire.co.uk

**Mobile Stables**

Timber sizes nominal before planning and processing, other dimensions may vary dependant on individual building.

**Harrier Range**

Ridge Height: 3.0m excluding Onduline

Eaves Height: 2.4m excluding Onduline

Threshold Height: 80mm

Opening Size: 1.880mm (w) x 2.090m (h) – from ground to top of opening is 2.170m

Overhang: 1050mm overhang lined with plywood (1200mm with gutter)

Skid: 80 x 40mm galvanised skid with towing points at either end

Framework: Constructed from 75x50mm cls tanalith E treated timber at 600mm centres. Studwork doubles at door apertures, additional cross members at 1.22m height.

Cladding: Premium ex19x125mm tanalith E treated overlap shiplap, fixed with 45mm sheradized ring shanked nails

Kick-boarding: Lined to 1.22m with 18mm OSB

Roof trusses: All trusses fixed to sections with 100mm or 150mm timber lock screws

Purlins: 100x50mm or 125x50mm positioned at a maximum of 600mm centres dependant on roof span

Roofing: Black Onduline with Onduline ridge capping lined with 11mm OSB

Guttering: 112mm black uPVC guttering fitted with 68mm downpipes to both ends of front elevation

Windows: Nil

Partition: ......................

Stable Doors Approx. 1220mm(w) x 2130(h) x 56mm (to fit 1230mm opening)

Constructed as follows:

* Top and Bottom door
* Clad with ex19x125mm V jointed tongue & grooved planed timber
* 150x28mm braced framework
* All ironmongery is hot dipped galvanised
* Heavy 600mm hinges
* 50mm chew strip to top of bottom door
* Lined internally with 12mm exterior grade plywood
* Brenton bolt to top door
* Kick-over latch
* Cabin hooks to both doors
* 200mm Auto animal bolt to bottom door
* Bottom door height 1200mm

**Mobile Combination units**

*(As mobile stable with the following differences for the Tack room section)*

Opening: Tackroom door width 0.90m wide x 2.1m high

Interior Lining: Unlined

Door: Supplied and fitted with three 16” T hinges, 6” Brenton bolt and cabin hook to secure door when open.

Floor: 100 x 50mm tanalith E treated joists at a maximum 600mm centres. Covered with 125x22mm sawn tanalith E treated floorboards or 18mm OSB

Roof lining: Face of truss between stable and tack room also boarded with 11mm OSB

**Mobile Tack room**

*(As mobile stable with the following differences)*

Interior Lining: All walls are fully lined to eaves height with 11mm OSB

Door: Supplied and fitted with three 16” T hinges, 6” Brenton bolt and cabin hook to secure door when open.

Floor: 100x50mm tanalith E treated joists at a maximum 600mm centres. Covered with 150 x 28mm sawn Tanalith E treated floorboards

Roof lining: 11mm OSB.