Tel



Tel: 01789 400988

Email: enquiries@redmire.co.uk

**Mobile Stables**

Timber sizes nominal before planning and processing, other dimensions may vary dependant on individual building.

**Hawk Range**

Eaves Height: 2.34m excluding Onduline

Ridge Height: 2.89m excluding Onduline

Threshold Height: 113mm

Opening Size: 1.880mm (w) x 2.010m (h) – from ground to top of opening is 2.143m

Overhang: 650mm overhang (3m deep models), 1.05m overhang (on 3.6m deep models)

Skid: 150x75mm tanalith E treated skid with galvanised steel towing points at either end

Framework: Constructed from 75x50mm cls tanalith E treated timber at 600mm centres. Studwork doubles at door apertures, additional cross members at 1.22m height.

Cladding: Premium ex16mm tanalith E treated overlap shiplap

Kick-boarding: Lined to 1.22m with 11mm OSB

Roof trusses: Constructed from 100x50mm Tanalith E Treated timber. All trusses fixed to sections with 100mm or 150mm timber lock screws

Purlins: 100x50mm positioned at a maximum of 550mm centres

Roofing: Black Onduline with Onduline ridge capping

Guttering: Nil

Windows: Nil

Partition: ......................

Stable Doors Approx. 1220mm(w) x 2130(h) x 56mm (to fit 1230mm opening)

Constructed as follows:

* Bottom door only
* Clad with ex19x125mm V jointed tongue & grooved planed timber
* 150x28mm braced framework
* All ironmongery is hot dipped galvanised
* Heavy 450mm hinges
* 50mm chew strip to top of bottom door
* Lined internally with 12mm exterior grade plywood
* Brenton bolt to top door
* Kick-over latch
* 200mm Auto animal bolt to bottom door
* Bottom door height 1200mm

**Mobile Combination units**

*(as field shelter with the following differences for the Tack room section)*

 Opening: Tackroom door width 0.9m wide x 2.1m high

 Interior Lining: Unlined

Door: Supplied and fitted with three 16” T hinges, 6” Brenton bolt and cabin hook to secure door when open.

Floor: 100x50mm tanalith E treated joists at a maximum 600mm centres. Covered with 18mm OSB floorboards

Roof lining: Face of truss between stable and tack room also boarded