[](http://www.redmire.co.uk/)

Tel: 01789 400988

Email: enquiries@redmire.co.uk

**Mobile Stables**

Timber sizes nominal before planning and processing, other dimensions may vary dependant on individual building.

**Hunter Range**

Ridge Height: 3.01m excluding Onduline

Eaves Height: 2.46m excluding Onduline

Threshold Height: 138mm

Opening Size: 1.22m (w) x 2.09m (h) – from ground to top of opening is 2.228m

Overhang: With 1.2m overhang lined with plywood (1.35m with gutter)

Skid: 100x100mm galvanised skid with towing points at either end

Framework: Constructed from 100x50mm cls tanalith E treated timber at 600mm centres. Studwork doubles at door apertures. Additional 100x50mm cls cross members at 1.22m height.

Cladding: Premium ex19x125mm tanalith E treated overlap shiplap, fixed with 45mm sheradized ring shanked nails

Kick-boarding: Lined to 1.22m with 12mm plywood

Roof trusses: All trusses fixed to sections with 100mm or 150mm timberlock screws

Purlins: 100x50mm or 125x50mm positioned at a maximum of 600mm centres dependant on roof span

Roofing: Black Onduline with Onduline ridge capping lined with 11mm OSB

Guttering: 112mm black upvc guttering fitted with one 68mm downpipe to either end of front elevation

Windows: Nil

Stable Doors Approx. 1220mm(w) x 2130(h) x 56mm (to fit 1230mm opening)

Constructed as follows:

* Top and Bottom door
* Clad with ex19x125mm V jointed tongue & grooved planed timber
* 150x28mm braced framework
* All ironmongery is hot dipped galvanised
* Heavy 600mm hinges
* 50mm chew strip to top of bottom door
* Top door frame protection fitted
* Lined internally with 12mm exterior grade plywood
* Brenton bolt to top door
* Kick-over latch
* Cabin hooks to both doors
* 200mm Auto animal bolt to bottom door
* Bottom door height 1200mm

**Mobile Combination units**

*(As mobile stable with the following differences for the tack room section)*

Opening: Tack room door width 0.90m wide x 2.1m high

Interior Lining: All walls are fully lined to eaves with 9mm hardwood faced ply

Door: Supplied and fitted with three 600mm T hinges, 150mm Brenton bolt and cabin hook to secure door when open.

Floor: 100x50mm tanalith E treated joists covered with 125x22mm sawn Tanalith E treated floorboards or 18mm OSB

Roof lining: Face of truss between stable and tack room also boarded with hardwood faced ply.

**Mobile Tack room**

*(As mobile stable with the following differences)*

Interior Lining: All walls are fully lined to eaves height with 9mm hardwood faced ply

Door: Supplied and fitted with three 24” T hinges, 6” Brenton bolt and cabin hook to secure door when open.

Floor: 100x50mm Tanalith E treated joists covered with 125 x 22mm sawn Tanalith E treated floorboards or 18mm OSB

Roof lining: 11mm OSB