|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Replacement doors | | **Heavy duty tee hinges** |  | **Hook and Band Hinges** |  | **Heavy Reversible Cup Hinges** |
|  |  |  |  |  |  |  |
| **Door Size** | **Hinge Size Frame** |  |  |
| (frame not included)  **Complete Stable Doors** |  |  |  |
| 1.10 x 2.10m | 24” £80.00 | £280.00 |  | £300.00 |  | £340.00 |
| 1.22 x 2.10m | 24” £80.00 | £280.00 |  | £300.00 |  | £340.00 |
|  |  |  |  |  |  |  |
| **Bottom Stable doors** |  |  |  |  |  |  |
| 1.10 x 1.20m | 24” £80.00 | £160.00 |  | £180.00 |  | £200.00 |
| 1.22 x 1.20m | 24” £80.00 | £160.00 |  | £180.00 |  | £200.00 |
|  |  |  |  |  |  |  |
| **Garage/ Barn Doors** |  |  |  |  |  |  |
| 1.80 x 2.10m | 24” £120.00 | £250.00 |  | £270.00 |  | £290.00 |
| 2.10 x 2.10m | 24” £120.00 | £300.00 |  | £320.00 |  | £340.00 |
| 2.40 x 2.10m | 24” £120.00 | £300.00 |  | £320.00 |  | £340.00 |
| 2.70 x 2.10m | 24” £120.00 | £300.00 |  | £320.00 |  | £340.00 |
|  |  |  |  |  |  |  |
| **Tack Room Doors** |  |  |  |  |  |  |
| 0.81 x 2.10m | 24” £80.00 | £140.00 |  | £160.00 |  | £180.00 |
| 0.90 x 2.10m | 24” £80.00 | £140.00 |  | £160.00 |  | £180.00 |
| 1.20 x 2.10m | 24” £80.00 | £180.00 |  | N/A |  |  |
|  |  |  |  |  |  |  |
| **Top Back doors** |  |  |  |  |  |  |
| 1.00 x 0.8m | 16” | £180.00 |  | £200.00 |  | £220.00 |
|  |  |  |  |  |  |  |
| **Top Stable doors** | 24’’ | £130.00 |  | £150.00 |  | £160.00 |

.

All Prices Subject To VAT

|  |  |  |  |
| --- | --- | --- | --- |
|  | | | |
|  |  | | |
|  |  | | |
|  |  | | |
| **2.4m Sliding door £900.00** | | | |
| Framed, ledged and braced (FLB) door POA | | | |
| Available with or without threshold, and includes door frame and 5 lever mortice lock: | | | |
| Casement doors. | | | |
| Are available in many sizes, with various options available for glazing. All are priced on application. | | | |
|  | | | |
| Windows | |  |  |
|  | |  |  |
| Hunter window. Fixed acrylic pane with fixed louvered vents. | | 0.6 x 0.9m | £120.00 |
| Heavy duty window grill. (to fit hunter window) | | --- |  |
| Casement windows. Glazed in 6.4mm laminated glass | | 1.2 x 1.05m |  |
|  | | 0.9 x 1.05m |  |
|  | | 0.625 x 0.9m |  |
| Double glazing for casement windows | | --- | P.O.A |

|  |  |
| --- | --- |
|  |  |
|  |  |
|  |
|  |