[](http://www.redmire.co.uk/)

Tel: 01403 785508

Email: enquiries@redmire.co.uk

**‘S’ Type Range – Hawk 2022**

**Delivery Only for DIY**

|  |  |
| --- | --- |
| Size (W x D) | Price |
| 2.4 x 1.8m | £705.00 |
| 3.0 x 1.8m | £865.00 |
| 3.6 x 1.8m | £1,045.00 |
|  |  |
| 2.4 x 2.4m | £730.00 |
| 3.0 x 2.4m | £910.00 |
| 3.6 x 2.4m | £1090.00 |
|  |  |
| 2.4 x 2.8m | £790.00 |
| 3.0 x 2.8m | £990.00 |
| 3.6 x 2.8m | £1,185.00 |

|  |  |
| --- | --- |
| **Optional Extras** |  |
| Metal gate | £135.00 |
| Ply Boarding for gate | £35.00 |
| Clear roof sheet | £30.00 |

# Timber sizes nominal before planning and processing, other dimensions may vary dependant on individual building.

**Mobile Field Shelter**

Front roof Height: 1.575m excluding skid

Rear roof Height: 1.375m excluding skid

Opening Size: 1.88m (w)

Overhang: Nil

Skid: 100x75mm tanalith E treated skid with galvanised steel towing points

Framework: Constructed from 75x50mm cls tanalith E treated timber at 600mm centres. Studwork doubles at door apertures

Cladding: Premium ex16mm Tanalith E treated overlap shiplap

Kick-boarding: Lined to 1.22m with 11mm OSB

Purlins: 100x50mm positioned at a maximum of 600mm centres

Roofing: Black Onduline un lined

Guttering: Nil